In the station of Langeland Distant Signal Repeaters are positioned in advance of the Exit Signals, so that the Aspect of the Main Signal can be seen for a second time. The small white Auxiliary Light indicates the reduced distance remaining to the Main Signal compared with the standard 1000m.
The following Main Signal is (still) displaying Stop: Immediately after passing the Distant Repeater Signal, press the Indusi-Alert (Enter-Key in Numeric Keypad) You should now be travelling no faster than about 40km/h.
The following Main Signal is displaying Proceed at Reduced Speed (40km/h): Immediately after passing the Distant Repeater Signal, press the Indusi-Alert (Enter-Key in Numeric Keypad) You should now be travelling no faster than about 70km/h.